Release note version

Contents

[RC38 2](#_Toc167441386)

[Improvement 2](#_Toc167441387)

[Bugs fixing 2](#_Toc167441388)

[RC51 2](#_Toc167441389)

[Improvement 2](#_Toc167441390)

[Bugs fixing 2](#_Toc167441391)

[RC53 2](#_Toc167441392)

[Improvement 2](#_Toc167441393)

# RC38

## Improvement

* [WebUI] - Addition of the GSM setting

## Bugs fixing

* [Back] – Charging session not stopped automatically if LSC power supply is removed and put again before timeout (XEV1R22T2ER)
* [Back] After power loss OCMF frame reason is "local", must be "power loss"

# RC51

## Improvement

* [Error 6mA] - Modification to harmonize EVCS behavior (after 4 fault detection => StopTransaction + faulted state until user action)
* [Error Overconsumption] - Modification to harmonize EVCS behavior (after 4 fault detection => StopTransaction + faulted state until user action)
* [WebUI] - Update submeters list names (« ECR140D / XEVA431 » + « ECR380D / XEVA433 »)
* [WebUI] - Allow inputs load shedding below 13A in 3P and 7A in 1P
* [WebUI] - Add a parameter to disable EV41 function
* [WebUI] - Changed the German languages word
* [WebUI] - Add APN requirements
* [LTE modem] - Make only one PIN code attempt after saving configuration
* [LTE modem] - Add connection status
* [LTE modem] - Add incorrect PIN code textbox
* [OCPP] - EV41SuspendChargingEnabled OCPP key added

## Bugs fixing

* [OCPP] - Websocket connection / disconnection in a loop
* [OCPP] - No automatic charging session restart after power failure
* [Update] - Update process duration reduced to 16min (applied for next update)

# RC53

## Improvement

* [Back] - /var/aux partition stay in read only state. I2P2 service does not accumulate messages anymore.

Bugs fixing